**OFFICIAL 2017 BID FORM:**

NOTICE TO INTERESTED BIDDERS FOR: (1) COUNTY PURCHASE OF SUPPLIES AND (2) COUNTY DEPOSITORIES

**Section 1. SUPPLIES**

 Notice is hereby given that the Board of Supervisors of Montgomery County, Mississippi, will accept sealed bids (FOB VENDOR FACILITY AND DELIVERED TO MONTGOMERY COUNTY) for and on behalf of the Montgomery County Unit System until 5:00 o’clock P.M. on Friday, December 1, 2017. Said bids will be opened at the 8:00 A.M. Regular December 4, 2017 Board of Supervisors Meeting, for the furnishing to said County of the following itemized supplies for the period beginning January 1, 2018 and ending December 31, 2019. Any questions call the Road Manager Chris Breazeale at 662-283-1172:

1. **ROAD CONSTRUCTION MATERIALS**:
2. **Wash Gravel-Stabilizer aggregate commercial course gravel, size no. 1**, as specified in Sub-Section S-1703.17c of the Mississippi Standard Specifications for the State Aid Road and Bridge Construction, 1971 Edition: **(Montgomery County reserves the right to test wash gravel in 1000 ton lots). Failure to meet specifications will result in a 20% below bid payment for said lot**;

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Pea Gravel**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_ Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Clay Gravel-Class 3 Granular Material** as specified in the Mississippi Standard Specifications for State Aid Road and Bridge Construction 1989 Edition: **(Montgomery County reserves the right to test clay gravel in 1000 ton lots). Failure to meet specifications will result in a 20% below bid payment for said lot**;

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Over-Size Gravel**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Limestone (610)**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Limestone (5)**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Limestone (7)**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Concrete Sand**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Hot Surface Mix Asphalt**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Standard Cold Mix Asphalt**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **High Performance Cold Mix Asphalt**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Ready Mix Concrete:** (Delivered with minimum of 3000 lb.)

 Five (5) Bag Strength: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Emulsions**: (Delivered)

 Prime EPR: \_\_\_\_\_\_\_\_\_\_\_\_CRS-2: \_\_\_\_\_\_\_\_\_\_\_CRS-2P: \_\_\_\_\_\_\_\_\_\_\_CSS1H:\_\_\_\_\_\_\_\_\_\_\_

1. **Rip-Rap (100 lb.)**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Rip-Rap (200 lb.)**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **Rip-Rap (300 lb.)**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **CFB Ash**:

 FOB Plant: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Location: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Delivered: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. **GRADER BLADES**: (5/8” thick, 5/8” bolt hole, 8” wide, 7’ long, square ends)
2. Price per linear foot: $\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
3. **OIL PRODUCTS**:
4. Unleaded Gasoline: $\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_
5. Diesel Fuel $\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 The Board reserves the right to reject any and all bids submitted!!!

Submitted by: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Company: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Phone: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_